MRatWork Forum by Mustafa Ramadhan - Kapasitas directory home kenapa kecil gini?

Sponsor:
Server and Web Integrator
Link:
6.5.0 or 7.0.0
Click for "How to install"
Donation/Sponsorship:
Kloxo-MR is open-source.
Donate and or Sponsorship always welcome.
Click to:

MRatWork Forum | Please login or register. | 2017-11-07, 22:10:14

- MRatWork Forum by Mustafa Ramadhan »
- Language Specific Discussions »
- Indonesia Users »
- Kapasitas directory home kenapa kecil gini?

« previous next »

- Print

Pages: [1] Go Down

### Author Topic: Kapasitas directory home kenapa kecil gini? (Read 2864 times)

0 Members and 1 Guest are viewing this topic.

#### amudy17

- Senior Member
- Posts: 246
- Karma: +0/-1

##### Kapasitas directory home kenapa kecil gini?

« on: 2014-08-26, 08:44:56 »
Mau tanya besarin kapasitas /home gimana ya?
Check attachment.... kok... /home cuman max 78GB padahal HD di server sebesar 150GB
Logged
Free, Fast and Secure CP => Kloxo-MR
Daily News Update => Click here to see website!

#### amudy17

- Senior Member
- Posts: 246
- Karma: +0/-1

##### Re: Kapasitas directory home kenapa kecil gini?

« Reply #1 on: 2014-08-26, 10:01:52 »
Code: [Select]

    [root@server ~]# sh /script/sysinfo

    A. Kloxo-MR: 7.0.0.b-2014082402

    B. OS: CentOS release 6.5 (Final) x86_64

    C. Apps:
       1. MySQL: mysql55-5.5.39-1.ius.el6.x86_64
       2. PHP: php53u-5.3.29-1.ius.el6.x86_64
       3. Httpd: httpd-2.2.27-1.mr.e6.x86_64
       4. Lighttpd: --uninstalled--
       5. Hiawatha: hiawatha-9.7.b-1.mr.el6.x86_64
       6. Nginx: nginx-1.7.4-1.el6.ngx.x86_64
       7. Cache: --uninstalled--
       8. Dns: bind-9.8.2-0.23.rc1.el6_5.1.x86_64
       9. Qmail: qmail-toaster-1.03-1.3.38.mr.el6.x86_64
          - with: courier-imap-toaster-4.1.2-1.3.16.mr.el6.x86_64

    D. Php-type (for Httpd/proxy): php-fpm_worker

    E. Memory:
                    total       used       free     shared    buffers     cached
       Mem:          7822       2576       5245          0        247       1217
       -/+ buffers/cache:       1111       6710
       Swap:         7951          0       7951

Logged
Free, Fast and Secure CP => Kloxo-MR
Daily News Update => Click here to see website!

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: Kapasitas directory home kenapa kecil gini?

« Reply #2 on: 2014-08-26, 20:08:42 »
Tergantung bagaimana server anda diatur partisinya.
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### amudy17

- Senior Member
- Posts: 246
- Karma: +0/-1

##### Re: Kapasitas directory home kenapa kecil gini?

« Reply #3 on: 2014-08-27, 04:11:15 »
oooalah oke deh pak ga papa kok... ntar tinggal tambah harddisk aja
Logged
Free, Fast and Secure CP => Kloxo-MR
Daily News Update => Click here to see website!

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: Kapasitas directory home kenapa kecil gini?

« Reply #4 on: 2014-08-27, 04:18:11 »
Informasikan 'cat /etc/fstab'
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### amudy17

- Senior Member
- Posts: 246
- Karma: +0/-1

##### Re: Kapasitas directory home kenapa kecil gini?

« Reply #5 on: 2014-08-27, 11:02:37 »
Code: [Select]

    [root@server ~]# cat /etc/fstab

    #
    # /etc/fstab
    # Created by anaconda on Wed Aug 20 13:30:23 2014
    #
    # Accessible filesystems, by reference, are maintained under '/dev/disk'
    # See man pages fstab(5), findfs(8), mount(8) and/or blkid(8) for more info
    #
    /dev/mapper/vg_server-lv_root /                       ext4    defaults        1 1
    UUID=386c1b79-d10a-4584-bea1-5eacbdc9b05e /boot                   ext4    defaults        1 2
    /dev/mapper/vg_server-lv_home /home                   ext4    defaults        1 2
    /dev/mapper/vg_server-lv_swap swap                    swap    defaults        0 0
    tmpfs                   /dev/shm                tmpfs   defaults        0 0
    devpts                  /dev/pts                devpts  gid=5,mode=620  0 0
    sysfs                   /sys                    sysfs   defaults        0 0
    proc                    /proc                   proc    defaults        0 0

pak MR, kalau saya tambah harddisk di server, perlu menambahkan perintah apa???
Logged
Free, Fast and Secure CP => Kloxo-MR
Daily News Update => Click here to see website!

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: Kapasitas directory home kenapa kecil gini?

« Reply #6 on: 2014-08-27, 11:28:50 »
Terlihat / dan / berbeda partisi.
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### amudy17

- Senior Member
- Posts: 246
- Karma: +0/-1

##### Re: Kapasitas directory home kenapa kecil gini?

« Reply #7 on: 2014-08-27, 11:43:52 »
maksudnya pak?
Logged
Free, Fast and Secure CP => Kloxo-MR
Daily News Update => Click here to see website!

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: Kapasitas directory home kenapa kecil gini?

« Reply #8 on: 2014-08-27, 11:49:22 »
'/dev/mapper/vg_server-lv_root' adalah partisi LVM untuk '/' dan '/dev/mapper/vg_server-lv_home' untuk untuk '/home'. Partisi untuk '/home' kemudian di-mount ke '/'.
Untuk lebih jelas anda bisa infokan 'fdisk -l'.
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### amudy17

- Senior Member
- Posts: 246
- Karma: +0/-1

##### Re: Kapasitas directory home kenapa kecil gini?

« Reply #9 on: 2014-08-27, 11:59:18 »
Code: [Select]

    [root@server ~]# fdisk -l

    Disk /dev/sda: 146.2 GB, 146163105792 bytes
    255 heads, 63 sectors/track, 17769 cylinders
    Units = cylinders of 16065 * 512 = 8225280 bytes
    Sector size (logical/physical): 512 bytes / 512 bytes
    I/O size (minimum/optimal): 512 bytes / 512 bytes
    Disk identifier: 0x000c5cbb

       Device Boot      Start         End      Blocks   Id  System
    /dev/sda1   *           1          64      512000   83  Linux
    Partition 1 does not end on cylinder boundary.
    /dev/sda2              64       17770   142224384   8e  Linux LVM

    Disk /dev/mapper/vg_server-lv_root: 53.7 GB, 53687091200 bytes
    255 heads, 63 sectors/track, 6527 cylinders
    Units = cylinders of 16065 * 512 = 8225280 bytes
    Sector size (logical/physical): 512 bytes / 512 bytes
    I/O size (minimum/optimal): 512 bytes / 512 bytes
    Disk identifier: 0x00000000

    Disk /dev/mapper/vg_server-lv_swap: 8338 MB, 8338276352 bytes
    255 heads, 63 sectors/track, 1013 cylinders
    Units = cylinders of 16065 * 512 = 8225280 bytes
    Sector size (logical/physical): 512 bytes / 512 bytes
    I/O size (minimum/optimal): 512 bytes / 512 bytes
    Disk identifier: 0x00000000

    Disk /dev/mapper/vg_server-lv_home: 83.6 GB, 83609255936 bytes
    255 heads, 63 sectors/track, 10164 cylinders
    Units = cylinders of 16065 * 512 = 8225280 bytes
    Sector size (logical/physical): 512 bytes / 512 bytes
    I/O size (minimum/optimal): 512 bytes / 512 bytes
    Disk identifier: 0x00000000

Logged
Free, Fast and Secure CP => Kloxo-MR
Daily News Update => Click here to see website!

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: Kapasitas directory home kenapa kecil gini?

« Reply #10 on: 2014-08-27, 12:02:37 »
- Disk /dev/mapper/vg_server-lv_home: 83.6 GB
- Disk /dev/mapper/vg_server-lv_root: 53.7 GB
Jelaskan?.
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### amudy17

- Senior Member
- Posts: 246
- Karma: +0/-1

##### Re: Kapasitas directory home kenapa kecil gini?

« Reply #11 on: 2014-08-27, 12:15:07 »
artinya terlalu banyak space pada root ya? lantas saya mesti gimana untuk mengurangi space root dan memindahkan ke partisi /home??
Logged
Free, Fast and Secure CP => Kloxo-MR
Daily News Update => Click here to see website!

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: Kapasitas directory home kenapa kecil gini?

« Reply #12 on: 2014-08-27, 12:16:22 »
Ya harus install lagi secara manual.
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### amudy17

- Senior Member
- Posts: 246
- Karma: +0/-1

##### Re: Kapasitas directory home kenapa kecil gini?

« Reply #13 on: 2014-08-29, 13:55:58 »
yawdah biar saja tinggal tambah harddisk lagi pak
Logged
Free, Fast and Secure CP => Kloxo-MR
Daily News Update => Click here to see website!

- Print

Pages: [1] Go Up
« previous next »

- MRatWork Forum by Mustafa Ramadhan »
- Language Specific Discussions »
- Indonesia Users »
- Kapasitas directory home kenapa kecil gini?

Top 10 Social Networking: Facebook Twitter LinkedIn Pinterest Google Plus Tumblr Instagram VK Flickr Vine

..:: Monetize Your Website with ylliXmedia ::.. ..:: Online Advertising that Sale Anything with ylliXmedia ::..

- Design By SMFSimple.com
- SMF 2.0.14 | SMF © 2017, Simple Machines

Page created in 0.039 seconds with 17 queries.

Mirror created by MasterkinG32.CoM