MRatWork Forum by Mustafa Ramadhan - error di ip

Sponsor:
Server and Web Integrator
Link:
6.5.0 or 7.0.0
Click for "How to install"
Donation/Sponsorship:
Kloxo-MR is open-source.
Donate and or Sponsorship always welcome.
Click to:

MRatWork Forum | Please login or register. | 2017-11-07, 19:02:01

- MRatWork Forum by Mustafa Ramadhan »
- Language Specific Discussions »
- Indonesia Users »
- error di ip

« previous next »

- Print

Pages: 1 [2] 3 Go Down

### Author Topic: error di ip (Read 7387 times)

0 Members and 1 Guest are viewing this topic.

#### prandah

- Senior Member
- Posts: 343
- Karma: +0/-0

##### Re: error di ip

« Reply #15 on: 2013-08-10, 04:54:50 »
halo sory baru bangun tidur
webmail.abenetworkshop.com
« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
Main Main Kesini

#### nusapenida

- Junior Member
- Posts: 30
- Karma: +0/-0

##### Re: error di ip

« Reply #16 on: 2013-08-10, 06:25:10 »
Quote from: "MRatWork"

> Tanda 'FastCGI: server "/home/admin/username/domain.com.0fake" stderr:' artinya php-fpm anda masih pakai ip-port dan seharusnya sudah ganti ke socket. Ini anda ada pakai file custom di apache dan atau php-fpm. File custom ini harus anda sesuaikan dengan file originalnya.

pak,
setelah cek, saya belum menggunakan custom file baik di apache, php-fpm ataupin di nginx (/home/apache/tpl)
ada solusi?
thanks
« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged

#### prandah

- Senior Member
- Posts: 343
- Karma: +0/-0

##### Re: error di ip

« Reply #17 on: 2013-08-11, 06:41:44 »
iya sama
kok aneh ya
Code: [Select]

    [Sun Aug 11 00:39:32 2013] [error] [client 192.254.73.242] (111)Connection refused: FastCGI: failed to connect to server "/home/xxxx/xxxx/xxxx.com.0fake": connect() failed

« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
Main Main Kesini

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: error di ip

« Reply #18 on: 2013-08-11, 06:52:10 »
Isi /home/php-fpm/sock sama tidak namanya (tidak termasuk extension) dengan /etc/php-fpm/conf.d
« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### prandah

- Senior Member
- Posts: 343
- Karma: +0/-0

##### Re: error di ip

« Reply #19 on: 2013-08-11, 07:53:26 »
gini isinya
Code: [Select]

    [root@pegasus ~]# dir /home/php-fpm/sock
    abe.sock       apache.sock    download.sock  jjomobi.sock   romneyks.sock
    admin.sock     blogbola.sock  homemade.sock  lishuiec.sock  techgela.sock
    animalia.sock  ditusuk.sock   homesdes.sock  rohan.sock
    [root@pegasus ~]# dir /etc/php-fpm/conf.d
    dir: cannot access /etc/php-fpm/conf.d: No such file or directory
    [root@pegasus ~]#

« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
Main Main Kesini

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: error di ip

« Reply #20 on: 2013-08-11, 08:18:31 »
Maaf, mestinya di '/etc/php-fpm.d'
« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### prandah

- Senior Member
- Posts: 343
- Karma: +0/-0

##### Re: error di ip

« Reply #21 on: 2013-08-11, 12:01:25 »
sory baru bales. keknya sama deh :
Code: [Select]

    [root@pegasus ~]# dir /etc/php-fpm.d
    abe.conf       blogbola.conf  download.conf  jjomobi.conf   romneyks.conf
    admin.conf     default.conf   homemade.conf  lishuiec.conf  techgela.conf
    animalia.conf  ditusuk.conf   homesdes.conf  rohan.conf     www.nonconf
    [root@pegasus ~]# dir /home/php-fpm/sock
    abe.sock       apache.sock    download.sock  jjomobi.sock   romneyks.sock
    admin.sock     blogbola.sock  homemade.sock  lishuiec.sock  techgela.sock
    animalia.sock  ditusuk.sock   homesdes.sock  rohan.sock
    [root@pegasus ~]#

    tapi anehnya internal error itu
    fix kalo di restart :)
    tapi masak mau di restart terus ya :)

« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
Main Main Kesini

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: error di ip

« Reply #22 on: 2013-08-11, 12:33:45 »
Apa yang perlu direstart?. Mestinya terkait webserver atau php-fpm. Coba saja perhatikan apa yang jadi masalah (webserver atau php-fpm).
« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### prandah

- Senior Member
- Posts: 343
- Karma: +0/-0

##### Re: error di ip

« Reply #23 on: 2013-08-11, 12:40:55 »
kemungkinan sih php-fpm
karena ketika saya restart-services
maka yg akan muncul
Code: [Select]

    Stopping php-fpm:                                          [FAILED]
    Starting php-fpm: [11-Aug-2013 13:10:22] ERROR: An another FPM instance seems to already listen on /home/php-fpm/sock/apache.sock
    [09-Aug-2013 13:30:38] ERROR: FPM initialization failed
                                                               [FAILED]

« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
Main Main Kesini

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: error di ip

« Reply #24 on: 2013-08-11, 13:40:14 »
Bisa jadi php-fpm instance lama (pakai ip-port) masih jalan kemudian dicoba restart php-fpm baru (pakai socket). Jelas conflict.
Coba jalankan:
Code: [Select]

    killall php-fpm
    service php-fpm restart

Jika tidak manjur, reboot.
« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### prandah

- Senior Member
- Posts: 343
- Karma: +0/-0

##### Re: error di ip

« Reply #25 on: 2013-08-11, 14:03:31 »
untuk cara fix nya gimana ya yang bener?
« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
Main Main Kesini

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: error di ip

« Reply #26 on: 2013-08-11, 14:06:47 »
Jika sesuai dugaan saya, cukup reboot maka akan beres.
« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### prandah

- Senior Member
- Posts: 343
- Karma: +0/-0

##### Re: error di ip

« Reply #27 on: 2013-08-11, 14:14:36 »
iya beres, mas
tapi bakal muncul internal error lagi lama kelamaan
« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
Main Main Kesini

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: error di ip

« Reply #28 on: 2013-08-11, 14:27:06 »
Quote from: "goblog"

> iya beres, mas
> tapi bakal muncul internal error lagi lama kelamaan

Mestinya tidak lagi sepanjang php-fpm sudah pakai socket. Yang perlu dicermati apakah di /etc/sysctl.conf ada 'fs.file-max = 209708'.
Jika belum ada tambahkan tapi jika ada lebih dari 1 maka hilang duplikasinya.
Parameter ini penting untuk php-fpm yang pakai socket dimana bila tidak ada maka website 'temporary unavailable'.
« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### prandah

- Senior Member
- Posts: 343
- Karma: +0/-0

##### Re: error di ip

« Reply #29 on: 2013-08-11, 14:54:41 »
nah saya kebetulan ada2 nih
Code: [Select]

    [root@pegasus ~]# cat /etc/sysctl.conf
    # Kernel sysctl configuration file for Red Hat Linux
    #
    # For binary values, 0 is disabled, 1 is enabled.  See sysctl(8) and
    # sysctl.conf(5) for more details.

    # Controls IP packet forwarding
    net.ipv4.ip_forward = 0

    # Controls source route verification
    net.ipv4.conf.default.rp_filter = 1

    # Do not accept source routing
    net.ipv4.conf.default.accept_source_route = 0

    # Controls the System Request debugging functionality of the kernel
    kernel.sysrq = 0

    # Controls whether core dumps will append the PID to the core filename.
    # Useful for debugging multi-threaded applications.
    kernel.core_uses_pid = 1

    # Controls the use of TCP syncookies
    net.ipv4.tcp_syncookies = 1

    # Disable netfilter on bridges.
    net.bridge.bridge-nf-call-ip6tables = 0
    net.bridge.bridge-nf-call-iptables = 0
    net.bridge.bridge-nf-call-arptables = 0

    # Controls the default maxmimum size of a mesage queue
    kernel.msgmnb = 65536

    # Controls the maximum size of a message, in bytes
    kernel.msgmax = 65536

    # Controls the maximum shared segment size, in bytes
    kernel.shmmax = 68719476736

    # Controls the maximum number of shared memory segments, in pages
    kernel.shmall = 4294967296
    fs.file-max = 209708
    fs.file-max = 209708
    [root@pegasus ~]#

so solusinya dihilangkan 1 ?
« Last Edit: 1970-01-01, 01:00:00 by Guest »
Logged
Main Main Kesini

- Print

Pages: 1 [2] 3 Go Up
« previous next »

- MRatWork Forum by Mustafa Ramadhan »
- Language Specific Discussions »
- Indonesia Users »
- error di ip

Top 10 Social Networking: Facebook Twitter LinkedIn Pinterest Google Plus Tumblr Instagram VK Flickr Vine

..:: Monetize Your Website with ylliXmedia ::.. ..:: Online Advertising that Sale Anything with ylliXmedia ::..

- Design By SMFSimple.com
- SMF 2.0.14 | SMF © 2017, Simple Machines

Page created in 0.038 seconds with 18 queries.

Mirror created by MasterkinG32.CoM