MRatWork Forum by Mustafa Ramadhan - IP baru tak muncul di Kloxo MR

Sponsor:
Server and Web Integrator
Link:
6.5.0 or 7.0.0
Click for "How to install"
Donation/Sponsorship:
Kloxo-MR is open-source.
Donate and or Sponsorship always welcome.
Click to:

MRatWork Forum | Please login or register. | 2017-11-07, 21:27:10

- MRatWork Forum by Mustafa Ramadhan »
- Language Specific Discussions »
- Indonesia Users »
- IP baru tak muncul di Kloxo MR

« previous next »

- Print

Pages: [1] Go Down

### Author Topic: IP baru tak muncul di Kloxo MR (Read 1513 times)

0 Members and 1 Guest are viewing this topic.

#### redpages

- Senior Member
- Posts: 316
- Karma: +0/-0

##### IP baru tak muncul di Kloxo MR

« on: 2016-03-09, 06:21:23 »
Dear masta,
Saya menambahkan IP baru di VPS, tapi saya cek di Kloxo IP baru tersebut tidak muncul. Kenapa ya?
Quote

> A. Kloxo-MR: 7.0.0.b-2015102301
> - Web: hiawatha-9.15.0-f.6.mr.el6.i686
> - PHP: php54s-5.4.42-1.ius.el6 (cgi mode)
> B. Plateform:
> - OS: CentOS release 6.7 (Final) i686
> - Hostname: server80.xbackbone.com
> C. Services:
> 1. MySQL: MariaDB-server-10.0.21-1.el6.i686
> 2. PHP:
> - Branch: php54-cli-5.4.45-1.ius.el6.i686
> - Used: --Use PHP Branch--
> 3. Httpd: --uninstalled--
> - PHP Type: [unknown]
> 4. Lighttpd: --uninstalled--
> 5. Hiawatha: --unused--
> 6. Nginx: nginx-1.9.5-1.el6.ngx.i386
> 7. Cache: --uninstalled--
> 8. Dns: nsd-4.1.5-1.mr.el6.i686
> 9. Qmail: qmail-toaster-1.03-1.3.55.mr.el6.i386
> - with: courier-imap-toaster-4.1.2-1.3.18.mr.el6.i386
> D. Memory:
> total used free shared buffers cached
> Mem: 1006 613 392 27 49 318
> -/+ buffers/cache: 245 760
> Swap: 1023 0 1023
> E. Disk Space:
> Filesystem Size Used Avail Use% Mounted on
> /dev/vda1 19G 5.9G 12G 34% /

Mohon pencerahannya, terima kasih
Logged

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: IP baru tak muncul di Kloxo MR

« Reply #1 on: 2016-03-09, 06:25:24 »
Sudah coba di 're-read IP' di panel?.
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### redpages

- Senior Member
- Posts: 316
- Karma: +0/-0

##### Re: IP baru tak muncul di Kloxo MR

« Reply #2 on: 2016-03-09, 10:07:03 »
hehe.. iya. uda berhasil dengan cara re-read tadi.
Ceritanya ini mau saya bikin https. Bagaimana cara agar default alamat menjadi HTTPS, maksudnya setiap orang mengetikkan alamat tersebut (http) secara otomatis berubah menjadi https. Adakah menu di kloxo MR?. Saya menggunakan Nginx sebagai webserver
Logged

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: IP baru tak muncul di Kloxo MR

« Reply #3 on: 2016-03-09, 11:36:15 »
Cari saja 'redirect' icon di domain terkait.
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### redpages

- Senior Member
- Posts: 316
- Karma: +0/-0

##### Re: IP baru tak muncul di Kloxo MR

« Reply #4 on: 2016-03-16, 23:04:54 »
saya tambah 1 IP baru lagi tapi saya re-read IP baru masih belum muncul. Saya cek di panel VPS ada 3 IP, tapi di IP Address Kloxo masih 2.
Adakah cara lain untuk re-read selain lewat menu kloxo?
Logged

#### MRatWork

- Administrator
- The Elite
- Posts: 15,381
- Karma: +112/-9
- Gender:

##### Re: IP baru tak muncul di Kloxo MR

« Reply #5 on: 2016-03-16, 23:09:22 »
Coba saja lihat pakai 'ifconfig' atau 'ip addr'. Tampil IP apa saja?.
Logged
..:: MRatWork (Mustafa Ramadhan Projects) ::..
-- Server/Web-integrator - Web Hosting (Kloxo-MR READY!) --

#### redpages

- Senior Member
- Posts: 316
- Karma: +0/-0

##### Re: IP baru tak muncul di Kloxo MR

« Reply #6 on: 2016-03-17, 00:36:26 »
ifconfig
Quote

> [root@server80 ~]# ifconfig
> eth0 Link encap:Ethernet HWaddr 00:16:3C:41:20:5F
> inet addr:192.3.90.108 Bcast:192.3.90.255 Mask:255.255.255.0
> inet6 addr: fe80::216:3cff:fe41:205f/64 Scope:Link
> UP BROADCAST RUNNING MULTICAST MTU:1500 Metric:1
> RX packets:89637 errors:0 dropped:449 overruns:0 frame:0
> TX packets:29844 errors:0 dropped:0 overruns:0 carrier:0
> collisions:0 txqueuelen:1000
> RX bytes:6494328 (6.1 MiB) TX bytes:33938542 (32.3 MiB)
> Interrupt:11 Base address:0x2000
> eth0:0 Link encap:Ethernet HWaddr 00:16:3C:41:20:5F
> inet addr:192.3.90.14 Bcast:192.3.90.255 Mask:255.255.255.0
> UP BROADCAST RUNNING MULTICAST MTU:1500 Metric:1
> Interrupt:11 Base address:0x2000
> lo Link encap:Local Loopback
> inet addr:127.0.0.1 Mask:255.0.0.0
> inet6 addr: ::1/128 Scope:Host
> UP LOOPBACK RUNNING MTU:65536 Metric:1
> RX packets:854 errors:0 dropped:0 overruns:0 frame:0
> TX packets:854 errors:0 dropped:0 overruns:0 carrier:0
> collisions:0 txqueuelen:0
> RX bytes:79968 (78.0 KiB) TX bytes:79968 (78.0 KiB)

ip addr
Quote

> 1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN
> link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
> inet 127.0.0.1/8 scope host lo
> inet6 ::1/128 scope host
> valid_lft forever preferred_lft forever
> 2: eth0: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc pfifo_fast state UP qlen 1000
> link/ether 00:16:3c:41:20:5f brd ff:ff:ff:ff:ff:ff
> inet 192.3.90.108/24 brd 192.3.90.255 scope global eth0
> inet 192.3.90.14/24 brd 192.3.90.255 scope global secondary eth0:0
> inet6 fe80::216:3cff:fe41:205f/64 scope link
> valid_lft forever preferred_lft forever

Logged

- Print

Pages: [1] Go Up
« previous next »

- MRatWork Forum by Mustafa Ramadhan »
- Language Specific Discussions »
- Indonesia Users »
- IP baru tak muncul di Kloxo MR

Top 4 Global Search Engines: Google Bing Baidu Yahoo

- Design By SMFSimple.com
- SMF 2.0.14 | SMF © 2017, Simple Machines

Page created in 0.05 seconds with 19 queries.

Mirror created by MasterkinG32.CoM